http://www.xrite.com/product_overview.aspx?Action=support&ID=757  Software downloads

Xrite Profile Maker 5.0.10 available here
http://www.xrite.com/product_overview.aspx?ID=757&Action=support&SoftwareID=931
  Mac PC file downloads here 

Eye 1 diagnostics - to make sure your Gretag, EFI Fiery, Xrite Spectro is working (also check that serial number of base is same as serial number of eye one as they are supposed to be matched up to each other.

In order to use Eye 1 Profile Maker 5 make sure you have attached Spectro.

Start the program.

Click on Measure - Choose the type of test chart to Measure, GRACoLCoated1_ISO12647-7_ControlStrip2009.txt 
	If you can't find it make sure you have copied it to your computer and choose Open at top of choices.

Use the Measuring Chart button
Measure a Document that you have previously printed off like the Xerox GRACOL Quality control document that has a embedded strip. 
	You will need the plastic guide that comes with the Spectrometer but not the white board.
	Measure the 2  Color strips labeled Digital Control Strip
Start the program, you want to measure Strip with gaps
	After successfully measuring the strips close and a window called Untitled will come up

Click on Calculating Comparing
	For Sample choose Untitled (its at the bottom of the drop down list)
	For Reference choose the GRAColCoated1_ISO12647-7_ControlStrip2009.txt that you previously saved to your desktop or downloads directory.

After you have done this the report is visible to the right of the color bars ,it might be an idea to start saving reports mentioning, 
Machine,paper,Relative Humidity, Temp, in the file name. Maybe even numbering them so one could learn what works better over time?

You should also write the Delta E variation on the measured sample.

For reference Delta E variation of 1 is barely perceptible to human eye, apparently women tend to have better perception than men. Delta 3 or less is generally acceptable to majority of population.